1. The agency uses standard decals, lettering and numbering on vehicles to provide a standard look to agency vehicles. No other decals, lettering, numbering or stickers (except for registration stickers and toll tags) are authorized on vehicles.
2. The [Surplus Property Coordinator](mailto:jgoodma@tfs.tamu.edu) in Hudson coordinates the procurement and placement of the authorized decals, lettering and numbers on new vehicles purchased by the agency.
3. Decal specifications used by the agency are as follows:
   * Round logo (same as agency patch) – using artwork and color codes provided by the agency Communications office
     + Exception – Law Enforcement Vehicles
       - Law Enforcement round logo (same as agency LE patch) – using artwork and color codes provided by the agency Communications office.
   * Standard size for most vehicles – 14”
   * Exceptions: For tractor/trailer rigs – 18”

For small /compact cars – 12” (only if necessary to fit door) For dozers – 8”

For cargo trailers – 24"

* + Center (left to right and top to bottom) on both front doors, adjusting as needed for door molding, contours, door handles, name plate (e.g. F150), etc.
  + For dozers only – place decal on each side, towards rear of dozer
  + For cargo trailers only
    - Front – Patch centered, 4" down from roof seam to top of patch decal
      * Web address "tfsweb.tamu.edu" will be centered on front only, 2" black height – non-reflective (top of letters 3" from bottom of patch decal)
    - Sides
      * The words "TEXAS A&M FOREST SERVICE", black color (non- reflective), centered on side (adjusting for doors, windows, etc.), 4" down from roof seam
      * Patch centered on wording, 4" between bottom of wording to top of patch decal.
    - Exception – fire prevention
      * Fire prevention campaign messaging may be placed on the rear of cargo trailers or wrapped entirely
    - Exception – Law Enforcement
      * Law Enforcement campaign messaging may be placed on the rear of cargo trailers or wrapped entirely
    - For Command Trailers only
      * Use of the Lone Star State IMT patch logo is authorized but must include the agency patch decal on the same side.
      * Use of the words "LONE STAR STATE INCIDENT MANAGEMENT

TEAM", black color, will be used with the IMT patch logo.

* + - * Decals should be sized appropriately to the respective size of the command trailer and adjusting for windows, doors, slide outs, antennas, etc.
  + Fonts - Helvetica LT Standard, Bold
  + Reflective material

1. Lettering and Numbering specifications used by the agency are as follows:
   * Vehicles and heavy equipment with fire responsibilities.
     + The word “FIRE”
       - Red color, all caps,
       - 4” height on each front door (below Decal when possible; move to left or right if needed to accommodate decal)
       - 3” height on rear of vehicle (upper left corner of tailgate on pickups and below the glass on SUV’s, driver’s side)
     + Unit number
       - Black color
       - 3” height on rear of vehicle (upper right corner of tailgate on pickups and below the glass on SUV’s, passenger side)
       - 3" height on both sides of vehicle front fenders (centered over front tire and just below the hood; adjust to accommodate seams, molding or name plate, etc.)
       - 3" height on driver side front bumper; white color
       - Place unit # on each side, towards front of dozer
         * For large cab dozers, place unit # on cab frame. Numbers will be 4" wide and 5" tall; stretching 23" top to bottom
       - Place unit # on front right cargo trailer, midway or above rock panel
       - Roof identification (for dozers, transports, engines, and fireline supervisor pickups)
         * Standard – 18”- 36" height in black on the roof for white roofs
         * Exception – 18”- 36" height in white on the roof for black roofs
         * Exception – 12”- 36" height in black on the roof for small dozers
     + Law Enforcement Vehicles
       - The words “STATE LAW ENFORCEMENT”
       - Black color
       - 2” height on rear of vehicle (centered and flush with the bottom)
   * All other Vehicles
     + Unit number
       - Black color
       - 3” height on rear of vehicle (upper right corner of tailgate on pickups and below the glass on SUV’s, passenger side)
   * Fonts - Helvetica LT Standard, Bold
   * Reflective material

CONTACT: [Chief Administrative Officer](mailto:ewall@tfs.tamu.edu), (979) 458-5799