|  |
| --- |
| * Check **vehicle body** for damage
 |
| * Check direction **signals**/emergency **flashers** for operation and for cracked/missing lenses
 |
| * Check **windows** to be sure they are free of ice, snow, frost, etc.
 |
| * Adjust all **mirrors** to fit the driver and minimize blind spots
 |
| * Verify vehicle **registration** is not expired
 |
| * Check vehicle **tires** and **wheels** for:
* Loose /missing lug nuts
* Oil residue on inside/outside of wheel
* Proper inflation and no bulges present
 |
| * Check **under vehicle** for:
* Signs of fluid leaks
* Loose or hanging components
 |
| * Check the **windshield wipers** and **washers**
 |
| * Tap the **horn** to verify it works
 |
| * Verify driver’s **floorboard** is clear of debris for safe operation
 |